Loopback Adaptor

Fixing the Mac Address

Click on the Loopback Adaptor in Network and Sharing Center to pop up the Status pane

Click on Properties button

Click on Networking tab

Click on Configure button

Click on Advanced tab

Click on Network Address property

Set the value to 02-FA-FA-FA-FA-FA